{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":7,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBLQ-CV3"]
[]
[]
[]
[]
["","","","","","EBLQ05CAV3","EBLQ07CAV3"]
["Sound pressure level","Heating","","Nom.","dBA","48 (8)","49 (8)"]
["","Cooling","","Nom.","dBA","48 (8)","50 (8)"]
["Refrigerant","GWP","","","","2,088","2,088"]
["","Charge","","","kg","1.30","1.45"]
["","Type","","","","R-410A","R-410A"]
["Operation range","Cooling","Ambient","Max.","°CDB","43.0","43.0"]
["","","","Min.","°CDB","10.0","10.0"]
["","","Water side","Max.","°C","22.0","22.0"]
["","","","Min.","°C","5.00 (5)","5.00 (5)"]
["","Heating","Water side","Max.","°C","55.0","55.0"]
["","","","Min.","°C","15 (4)","15 (4)"]
["","Domestic hot water","Water side","Max.","°C","80 (7)","80 (7)"]
["","","","Min.","°C","25","25"]
["","","Ambient","Min.","°CDB","-25.0 (6)","-25.0 (6)"]
["","","","Max.","°CDB","35.0 (6)","35.0 (6)"]
["Cooling capacity","Nom.","","","kW","3.88 (1), 3.99 (2)","5.20 (1), 5.15 (2)"]
["Power input","Cooling","","Nom.","kW","0.950 (1), 1.93 (2)","1.37 (1), 2.69 (2)"]
["","Heating","","Nom.","kW","0.880 (1), 1.13 (2)","1.55 (1), 2.45 (2)"]
["Sound power level","Heating","","Nom.","dBA","61","62"]
["","Cooling","","Nom.","dBA","63.0","63.0"]
["COP","","","","","5.00 (1), 3.58 (2)","4.52 (1), 3.42 (2)"]
["Dimensions","Unit","","Width","mm","1,090","1,090"]
["","","","Depth","mm","350","350"]
["","","","Height","mm","735","735"]
["Weight","Unit","","","kg","76.0","80.0"]
["Space heating","Average climate water outlet 35°C","General","ηs (Seasonal space heating efficiency)","%","175","164"]
["","","","Seasonal space heating eff. class","","A++","A++"]
["","","","SCOP","","4.45","4.18"]
["","Average climate water outlet 55°C","General","Seasonal space heating eff. class","","A++","A++"]
["","","","ηs (Seasonal space heating efficiency)","%","126","126"]
["","","","SCOP","","3.22","3.22"]
["Fan","Air flow rate","Heating","High","m³/min","45.0","47.0"]
["","","Cooling","High","m³/min","52.5","52.5"]
["EER","","","","","4.07 (1), 2.07 (2)","3.80 (1), 2.10 (2)"]
["Heating capacity","Nom.","","","kW","4.40 (1), 4.03 (2)","7.00 (1), 6.90 (2)"]
["Power supply","Phase","","","","1~","1~"]
["","Name","","","","V3","V3"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","230","230"]
["Notes","","","","","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Condition 1: cooling Ta 35°C - LWE 18°C (DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )","(2) - Condition 2: cooling Ta 35°C - LWE 7°C ( DT = 5°C); heating Ta DB/WB 7°C/6°C - LWC 45°C ( DT = 5°C )"]
["","","","","","(3) - PED unit category: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(3) - PED unit category: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC"]
["","","","","","(4) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C","(4) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C"]
["","","","","","(5) - For more details on standard accessories refer to Installation/operation manual","(5) - For more details on standard accessories refer to Installation/operation manual"]
["","","","","","(6) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range.","(6) - Operation range domestic hot water (outdoor unit): range increase by support booster heater or backup heater. See separate drawing for operation range."]
["","","","","","(7) - > 50°C BSH only, no heatpump operation","(7) - > 50°C BSH only, no heatpump operation"]
["","","","","","(8) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information.","(8) - The sound pressure level is measured via a microphone at a certain distance from the unit. It is a relative value depending on the distance and acoustic environment. Refer to sound spectrum drawing for more information."]
["","","","","","(9) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(9) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation)."]
["","","","","","(10) - Including piping + PHE; excluding expansion vessel","(10) - Including piping + PHE; excluding expansion vessel"]
["","","","","","(11) - Daikin Altherma inverter controlled compressor starting current always <= max. running current","(11) - Daikin Altherma inverter controlled compressor starting current always <= max. running current"]