{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FBA35A2VEB / FBA35A2VEB / RZASG71M2V1B","FBA71A2VEB / RZASG71M2V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZASG140M7V1B","FBA35A2VEB / FBA35A2VEB / FBA35A2VEB / RZASG100M7V1B (Archived)","FBA50A2VEB / FBA50A2VEB / RZASG100M7V1B (Archived)"]
["Cooling capacity","Nom.","","kW","6.80 (1)","6.80 (1)"]
["Space cooling","SEER","","","5.43","6.19"]
["","Annual energy consumption","","kWh/a","438","385"]
["","Capacity","Pdesign","kW","6.80","6.80"]
["","Energy efficiency class","","","A","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.50","4.50"]
["","SCOP/A","","","3.82","4.01"]
["","Energy efficiency class","","","A","A+"]
["","Annual energy consumption","","kWh/a","1,649","1,571"]
["Heating capacity","Nom.","","kW","7.50 (2)","7.50 (2)"]
["Notes","","","","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Outdoor unit","","","","","","RZASG140M7V1B","RZASG100M7V1B","RZASG100M7V1B"]
["Cooling capacity","Nom.","","kW","","","13.4","9.50","9.50"]
["Heating capacity","Nom.","","kW","","","15.5","10.8","10.8"]
["Space cooling","Capacity","Pdesign","kW","","","13.4","9.50","9.50"]
["","SEER","","","","","9.67","5.31","5.38"]
["","Annual energy consumption","","kWh/a","","","832","626","618"]
["Space heating (Average climate)","Capacity","Pdesign","kW","","","7.80","6.00","6.00"]
["","SCOP/A","","","","","5.62","3.80","3.80"]
["","Annual energy consumption","","kWh/a","","","1943","2211","2211"]
["Space cooling","Energy efficiency class","","","","","","A","A"]
["Space heating (Average climate)","Energy efficiency class","","","","","","A","A"]