{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG60BVEB / RXS60L2V1B"]
["Cooling capacity","Nom.","","kW","5.70"]
["Heating capacity","Nom.","","kW","7.00"]
["Nominal efficiency","Annual energy consumption","","kWh","820"]
["","COP","","","3.52"]
["","EER","","","3.48"]
["","Energy labeling Directive","Cooling","","A"]
["","","Heating","","B"]
["Space cooling","Annual energy consumption","","kWh/a","321"]
["","Energy efficiency class","","","A++"]
["","Capacity","Pdesign","kW","5.70"]
["","SEER","","","6.22"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","1,646"]
["","Capacity","Pdesign","kW","4.71"]
["","Energy efficiency class","","","A+"]
["","Pdh Heating capacity at -10°","","kW","4.11"]
["","SCOP/A","","","4.00"]
["Piping connections","Drain","OD","mm","VP25 (External dia.32, internal dia. 25)"]
["","Gas","OD","mm","12.70"]
["","Liquid","OD","mm","6.35"]
["Notes","","","","(1) - When normally running: +22°C / + 32°C"]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data"]