{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":13,"n_cols":9,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FD-K5 / RU-K5"]
[]
[]
[]
[]
["","","","","FD06KY1 / RU06KY1","FD08KY1 / RU08KY1","FD10KY1 / RU10KY1","FD15KY1 / RU08KY1+RU08KY1","FD20KY1 / RU10KY1+RU10KY1"]
["Cooling capacity","Nom.","","kW","17.4 (1)","24.3 (1)","29.7 (1)","48.6 (1)","59.3 (1)"]
["Piping connections","Liquid","OD","mm","9.52","12.7","15.9","12.7","15.9"]
["","Gas","OD","mm","19.1","25.4","31.8","25.4","31.8"]
["","Drain","OD","mm","PT 3/4 internal thread","PT 3/4 internal thread","PT 3/4 internal thread","FPS1B","FPS1B"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal)","(1) - Cooling: indoor temp. 27°CDB, 19.5°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m (horizontal)"]
["","","","","(2) - Capacities are gross capacities which do not include a deduction for evaporator fan motor heat.","(2) - Capacities are gross capacities which do not include a deduction for evaporator fan motor heat.","(2) - Capacities are gross capacities which do not include a deduction for evaporator fan motor heat.","(2) - Capacities are gross capacities which do not include a deduction for evaporator fan motor heat.","(2) - Capacities are gross capacities which do not include a deduction for evaporator fan motor heat."]
["","","","","","","","(3) - Each value for outdoor unit shows the specification per one unit","(3) - Each value for outdoor unit shows the specification per one unit"]