{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FD-K5"]
[]
[]
[]
[]
["","","","","FD06KY1","FD08KY1","FD10KY1","FD15KY1","FD20KY1"]
["Sound pressure level","Cooling","Nom.","dBA","51","51","53","58","60"]
["Dimensions","Unit","Width","mm","1,130","1,130","1,330","1,620","1,980"]
["","","Depth","mm","850","850","850","850","850"]
["","","Height","mm","450","500","500","625","625"]
["Casing","Material","","","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel","Galvanised steel"]
["Weight","Unit","","kg","79","93","104","161","187"]
["Fan","External static pressure","Nom.","Pa","9","10","10","15","15"]
["Power supply","Phase","","","3~","3~","3~","3~","3~"]
["","Name","","","Y1","Y1","Y1","Y1","Y1"]
["","Frequency","","Hz","50","50","50","50","50"]
["","Voltage","","V","380-415","380-415","380-415","380-415","380-415"]