{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":81,"n_cols":14,"rows_kept":81,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-A"]
[]
[]
[]
[]
["","","","","","FTXF20A2V1B","FTXF20A5V1B","FTXF25A2V1B","FTXF25A5V1B","FTXF35A2V1B","FTXF35A5V1B","FTXF50A2V1B","FTXF60A2V1B","FTXF71A2V1B"]
["Sound pressure level","Heating","","High","dBA","39","39","40","40","40","40"]
["","","","Medium","dBA","34","34","34","34","35","35"]
["","","","Silent operation","dBA","21","21","21","21","21","21"]
["","","","Low","dBA","28","28","28","28","29","29"]
["","Cooling","","Medium","dBA","33","33","33","33","34","34"]
["","","","Silent operation","dBA","20","20","20","20","20","20"]
["","","","Low","dBA","25","25","26","26","27","27"]
["","","","High","dBA","39","39","40","40","43","43"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1","1","1"]
["","Infrared remote control","","","","1","1","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2","2","2"]
["","Remote control holder","","","","1","1","1","1","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2","2","2"]
["Control systems","Wired remote control","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.50","9.50","9.50","9.50","9.50","9.50"]
["","Drain","","","","18","18","18","18","18","18"]
["Power input","Cooling","","Nom.","kW","0.017","0.017","0.019","0.019","0.032","0.032"]
["","Heating","","Nom.","kW","0.020","0.020","0.020","0.020","0.032","0.032"]
["Sound power level","Cooling","","","dBA","55","55","55","55","58","58"]
["","Heating","","","dBA","55","55","55","55","58","58"]
["Dimensions","Unit","","Width","mm","770","770","770","770","770","770"]
["","","","Depth","mm","225","225","225","225","225","225"]
["","","","Height","mm","286","286","286","286","286","286"]
["Casing","Colour","","","","White","White","White","White","White","White"]
["Weight","Unit","","","kg","9.00","9.00","9.00","9.00","9.00","9.00"]
["Fan","Air flow rate","Heating","High","m³/min","10.3","10.3","10.3","10.3","11.5","11.5"]
["","","","Medium","m³/min","8.4","8.4","8.6","8.6","9.0","9.0"]
["","","","Low","m³/min","6.5","6.5","6.7","6.7","7.0","7.0"]
["","","","Silent operation","m³/min","5.3","5.3","5.3","5.3","5.3","5.3"]
["","","Cooling","Low","m³/min","5.9","5.9","6.1","6.1","6.3","6.3"]
["","","","Medium","m³/min","7.9","7.9","8.1","8.1","8.3","8.3"]
["","","","High","m³/min","9.8","9.8","10.1","10.1","11.5","11.5"]
["","","","Silent operation","m³/min","4.4","4.4","4.4","4.4","4.5","4.5"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Power input","Cooling","","Nom.","kW","","","","","","","0.029","0.032","0.032"]
["","Heating","","Nom.","kW","","","","","","","0.032","0.035","0.035"]
["Casing","Colour","","","","","","","","","","White","White","White"]
["Dimensions","Unit","","Height","mm","","","","","","","295","295","295"]
["","","","Width","mm","","","","","","","990","990","990"]
["","","","Depth","mm","","","","","","","263","263","263"]
["Weight","Unit","","","kg","","","","","","","13.5","13.5","13.5"]
["Fan","Air flow rate","Cooling","High","m³/min","","","","","","","16.8","17.3","17.3"]
["","","","Medium","m³/min","","","","","","","14.4","14.8","14.8"]
["","","","Low","m³/min","","","","","","","11.9","12.2","12.2"]
["","","","Silent operation","m³/min","","","","","","","10.5","10.7","10.7"]
["","","Heating","High","m³/min","","","","","","","17.3","17.9","17.9"]
["","","","Medium","m³/min","","","","","","","14.8","15.8","15.8"]
["","","","Low","m³/min","","","","","","","12.2","12.8","12.8"]
["","","","Silent operation","m³/min","","","","","","","10.7","11.3","11.3"]
["Sound power level","Cooling","","","dBA","","","","","","","59","60","62"]
["","Heating","","","dBA","","","","","","","61","62","62"]
["Sound pressure level","Cooling","","High","dBA","","","","","","","43","45","46"]
["","","","Medium","dBA","","","","","","","39","41","42"]
["","","","Low","dBA","","","","","","","34","36","37"]
["","","","Silent operation","dBA","","","","","","","31","33","34"]
["","Heating","","High","dBA","","","","","","","42","44","45"]
["","","","Medium","dBA","","","","","","","38","40","41"]
["","","","Low","dBA","","","","","","","33","35","36"]
["","","","Silent operation","dBA","","","","","","","30","32","33"]
["Piping connections","Liquid","","OD","mm","","","","","","","6.35","6.35","6.35"]
["","Gas","","OD","mm","","","","","","","12.7","12.7","12.7"]
["","Drain","","","","","","","","","","18","18","18"]
["Control systems","Infrared remote control","","","","","","","","","","ARC470A1","ARC470A1","ARC470A1"]
["","Wired remote control","","","","","","","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standard Accessories","Titanium apatite deodorizing filter","","","","","","","","","","2","2","2"]
["Power supply","Name","","","","","","","","","","V1","V1","V1"]
["","Phase","","","","","","","","","","1~","1~","1~"]
["","Frequency","","","Hz","","","","","","","50","50","50"]
["","Voltage","","","V","","","","","","","220-240","220-240","220-240"]