{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B"]
["Cooling capacity","Nom.","","kW","4.00","4.00","4.0","4.00","5.20","4.00","6.00"]
["Space cooling","SEER","","","7.62","7.46","7.62","7.72","7.70","5.42","6.23"]
["","Annual energy consumption","","kWh/a","164","188","164","182","237","258","337"]
["","Capacity","Pdesign","kW","4.00","4.00","4.00","4.00","5.20","4.00","6.00"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.80","5.00","4.80","4.80","5.00","3.20","5.30"]
["","SCOP/A","","","4.11","4.18","4.11","4.11","4.18","3.87","4.00"]
["","Energy efficiency class","","","A+","A+","A+","A+","A+","A","A+"]
["","Pdh Heating capacity at -10°","","kW","3.58","1.00","3.8","1.0","1.0","2.80","4.13"]
["","Annual energy consumption","","kWh/a","1,632","1,672","1,632","1,632","1,672","1,157","1,852"]
["Nominal efficiency","Annual energy consumption","","kWh","482","467","482","471","593","457","787"]
["","EER","","","4.15","4.28","4.15","4.25","4.38","4.38","3.81"]
["","COP","","","3.95","4.32","3.95","4.05","4.42","4.04","3.88"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","4.60","4.60","4.60","6.80","6.80","6.50","7.80"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series. Eurovent 2015 tolerances are used."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data"]