{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 2MXM-M"]
[]
[]
[]
[]
["","","","","FTXM20N2V1B / FTXM20N2V1B / 2MXM40M4V1B","FTXM20N2V1B / FTXM25N2V1B / 2MXM40M4V1B","FTXM20N2V1B / FTXM35N2V1B / 2MXM40M4V1B","FTXM25N2V1B / FTXM25N2V1B / 2MXM40M4V1B","FTXM25N2V1B / FTXM35N2V1B / 2MXM40M4V1B"]
["Cooling capacity","Nom.","","kW","4.00","4.00","4.00","4.00","4.00"]
["Space cooling","SEER","","","8.53","8.50","8.19","8.36","8.11"]
["","Annual energy consumption","","kWh/a","165","165","171","168","173"]
["","Capacity","Pdesign","kW","4.00","4.00","4.00","4.00","4.00"]
["","Energy efficiency class","","","A+++","A+++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","3.20","3.20","3.20","3.20","3.20"]
["","SCOP/A","","","4.64","4.60","4.60","4.60","4.61"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","2.55","2.56","2.58","2.57","2.59"]
["","Annual energy consumption","","kWh/a","966","973","974","974","971"]
["Nominal efficiency","Annual energy consumption","","kWh","485","481","476","478","472"]
["","EER","","","4.12","4.16","4.20","4.18","4.24"]
["","COP","","","4.28","4.32","4.41","4.37","4.46"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","4.20","4.20","4.20","4.20","4.20"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]