{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-N / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXM20N2V1B / FTXM20N2V1B / 3MXM40N2V1B","FTXM25N2V1B / FTXM25N2V1B / 3MXM52N2V1B","FTXM20N2V1B / FTXM20N2V1B / FTXM25N2V1B / 3MXM68N2V1B","FTXM20N2V1B / FTXM25N2V1B / FTXM25N2V1B / 3MXM68N2V1B","FTXM20N2V1B / FTXM50N2V1B / 3MXM68N2V1B","FTXM25N2V1B / FTXM42N2V1B / 3MXM68N2V1B","FTXM35N2V1B / FTXM35N2V1B / 3MXM68N2V1B"]
["Cooling capacity","Nom.","","kW","4.00","5.0","6.5","6.8","6.8","6.7","6.8"]
["Space cooling","SEER","","","8.52","8.59","7.76","7.71","7.78","7.99","8.02"]
["","Annual energy consumption","","kWh/a","165","204","294","309","306","294","297"]
["","Capacity","Pdesign","kW","4.00","5.00","6.50","6.80","6.80","6.70","6.80"]
["","Energy efficiency class","","","A+++","A+++","A++","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.80","4.80","5.30","5.30","4.50","4.30","4.80"]
["","SCOP/A","","","4.24","4.38","4.09","4.10","3.90","3.86","4.00"]
["","Energy efficiency class","","","A+","A+","A+","A+","A","A","A+"]
["","Pdh Heating capacity at -10°","","kW","3.60"]
["","Annual energy consumption","","kWh/a","1,582","1,533","1,814","1,807","1,612","1,559","1,680"]
["Nominal efficiency","Annual energy consumption","","kWh","420","515","810","883","794","751","723"]
["","EER","","","4.76","4.85","4.01","3.85","4.28","4.46","4.70"]
["","COP","","","4.73","4.45","4.49","4.38","3.82","3.95","3.81"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","4.60","6.80","8.20","8.60","8.60","8.30","8.60"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]