{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F / RXS-L"]
[]
[]
[]
[]
["","","","","FVXS25FV1B / RXS25L2V1B","FVXS35FV1B / RXS35L2V1B","FVXS50FV1B / RXS50L2V1B"]
["Cooling capacity","Min.","","kW","1.3","1.4","1.4"]
["","Max.","","kW","3.0","3.8","5.6"]
["","Nom.","","kW","2.5","3.5","5.0"]
["Space cooling","SEER","","","5.74","5.60","5.89"]
["","Annual energy consumption","","kWh/a","152","219","297"]
["","Capacity","Pdesign","kW","2.50","3.50","5.00"]
["","Energy efficiency class","","","A+","A+","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","2.60","2.90","4.20"]
["","SCOP/A","","","4.56","3.93","3.80"]
["","Energy efficiency class","","","A+","A","A"]
["","Annual energy consumption","","kWh/a","798","1,033","1,546"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","9.5","9.5","12.7"]
["","Drain","OD","mm","20.0","20.0","20"]
["Nominal efficiency","Annual energy consumption","","kWh","285","510","775"]
["","EER","","","4.39","3.43","3.23"]
["","COP","","","4.42","3.78","3.63"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Heating capacity","Nom.","","kW","3.4","4.5","5.8"]
["","Min.","","kW","1.3","1.4","1.4"]
["","Max.","","kW","4.5","5.0","8.1"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V"]
["","","","","(5) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(5) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m","(5) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB, 24°CWB; equivalent piping length: 5m"]
["","","","","(6) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(6) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m","(6) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 5m"]
["","","","","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(7) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]