{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":13,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWF-BT"]
[]
[]
[]
[]
["","","","","","FWF02B5TV1B","FWF02B7TV1B","FWF03B5TV1B","FWF03B7TV1B","FWF04B5TV1B","FWF04B7TV1B","FWF05B7TV1B","FWF05B5TV1B"]
["Sound pressure level","Super high","","","dBA","","31","","31","","40","45"]
["","Low","","","dBA","26.0","26","26.0","26","26.0","26","30","30.0"]
["","High","","","dBA","31.0","27","31.0","27","40.0","33","39","45.0"]
["Standard Accessories","Installation and operation manual","","","","1","Installation and operation manual","1","Installation and operation manual","1","Installation and operation manual","Installation and operation manual","1"]
["","Drain hose","","","","1","Drain hose","1","Drain hose","1","Drain hose","Drain hose","1"]
["","Clamp for drain hose","","","","1","Clamp for drain hose","1","Clamp for drain hose","1","Clamp for drain hose","Clamp for drain hose","1"]
["","Washer for hanger bracket","","","","8","Washer for hanger bracket","8","Washer for hanger bracket","8","Washer for hanger bracket","Washer for hanger bracket","8"]
["","Screws","","","","4","Screws","4","Screws","4","Screws","Screws","4"]
["","Installation guide","","","","1","Installation guide","1","Installation guide","1","Installation guide","Installation guide","1"]
["","O ring","","","","2","O ring","2","O ring","2","O ring","O ring","2"]
["","Insulation","","","","6","Insulation","6","Insulation","6","Insulation","Insulation","6"]
["Control systems","Wired remote control","","","","","BRC315D7","","BRC315D7","","BRC315D7","BRC315D7"]
["","Infrared remote control","","","","","BRC7E530, BRC7E531","","BRC7E530, BRC7E531","","BRC7E530, BRC7E531","BRC7E530, BRC7E531"]
["Total sound power level","Low","","","dBA","36.0","","38.0","","38.0","","","42.0"]
["","High","","","dBA","44.0","","44.0","","50.0","","","55.0"]
["Water flow","Water pressure drop","Heating","High","kPa","7","","18","","30","","","43"]
["","","Cooling","High","kPa","5","","17","","29","","","40"]
["Piping connections","Drain","","OD","mm","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)","VP20 (External dia.26, Internal dia. 20)"]
["","Water","","Inlet","","3/4\" BSP (female thread)","3/4\" BSP (female thread)","3/4\" BSP (female thread)","3/4\" BSP (female thread)","3/4\" BSP (female thread)","3/4\" BSP (female thread)","3/4\" BSP (female thread)","3/4\" BSP (female thread)"]
["","","","Outlet","","3/4\" BSP (female thread)","3/4\" BSP (female thread)","3/4\" BSP (female thread)","3/4\" BSP (female thread)","3/4\" BSP (female thread)","3/4\" BSP (female thread)","3/4\" BSP (female thread)","3/4\" BSP (female thread)"]
["Power input","High","","","kW","0.074","","0.074","","0.090","","","0.118"]
["","Low","","","kW","0.060","","0.060","","0.055","","","0.062"]
["Allowed water temperature","Heating","","Max.","°C","50 (5)","","50 (5)","","50 (5)","","","50 (5)"]
["","","","Min.","°C","5 (5)","","5 (5)","","5 (5)","","","5 (5)"]
["","Cooling","","Min.","°C","5 (5)","","5 (5)","","5 (5)","","","5 (5)"]
["","","","Max.","°C","50 (5)","","50 (5)","","50 (5)","","","50 (5)"]
["Dimensions","Unit","","Width","mm","575","575","575","575","575","575","575","575"]
["","","","Depth","mm","575","575","575","575","575","575","575","575"]
["","","","Height","mm","285 (4)","285","285 (4)","285","285 (4)","285","285","285 (4)"]
["Weight","Unit","","","kg","19","19","19","19","19","19","19","19"]
["Fan","Air flow rate","","Low","m³/h","300","318","318","318","318","318","420","420"]
["","","","High","m³/h","456","468","468","468","660","660","876","876"]
["Cooling capacity (standard conditions)","Sensible capacity 2-pipe","","Low","kW","1.0 (1)","","1.4 (1)","","1.4 (1)","","","1.8 (1)"]
["","","","High","kW","1.4 (1)","","2.0 (1)","","2.7 (1)","","","3.5 (1)"]
["","Total capacity 2-pipe","","Low","kW","1.3 (1)","","2.4 (1)","","2.4 (1)","","","2.8 (1)"]
["","","","High","kW","1.7 (1)","","3.0 (1)","","4.0 (1)","","","4.9 (1)"]
["Heating capacity (standard conditions)","Capacity 2-pipe","","High","kW","2.4 (2)","","3.3 (2)","","4.5 (2)","","","5.6 (2)"]
["","","","Low","kW","1.9 (2)","","2.7 (2)","","2.7 (2)","","","3.0 (2)"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50","50","50","50"]
["","Voltage","","","V","220-440","220-440","220-440","220-440","220-440","220-440","220-440","220-440"]
["Notes","","","","","(1) - Cooling: air 27°CDB, 19°CWB; entering water 7°C; leaving water 12°C","(1) - Cooling: air 27°CDB, 19°CWB; entering water 7°C; leaving water 12°C","(1) - Cooling: air 27°CDB, 19°CWB; entering water 7°C; leaving water 12°C","(1) - Cooling: air 27°CDB, 19°CWB; entering water 7°C; leaving water 12°C","(1) - Cooling: air 27°CDB, 19°CWB; entering water 7°C; leaving water 12°C","(1) - Cooling: air 27°CDB, 19°CWB; entering water 7°C; leaving water 12°C","(1) - Cooling: air 27°CDB, 19°CWB; entering water 7°C; leaving water 12°C","(1) - Cooling: air 27°CDB, 19°CWB; entering water 7°C; leaving water 12°C"]
["","","","","","(2) - Heating: 2 pipe: air 20°CDB, 15°CWB; entering water 45°C; leaving water 40°C","(2) - Heating: 2 pipe: air 20°CDB; entering water 50°C","(2) - Heating: 2 pipe: air 20°CDB, 15°CWB; entering water 45°C; leaving water 40°C","(2) - Heating: 2 pipe: air 20°CDB; entering water 50°C","(2) - Heating: 2 pipe: air 20°CDB, 15°CWB; entering water 45°C; leaving water 40°C","(2) - Heating: 2 pipe: air 20°CDB; entering water 50°C","(2) - Heating: 2 pipe: air 20°CDB; entering water 50°C","(2) - Heating: 2 pipe: air 20°CDB, 15°CWB; entering water 45°C; leaving water 40°C"]
["","","","","","(3) - Heating: 4 pipe: air 20°CDB, 15°CWB; entering water 65°C; leaving water 55°C","(3) - Do not let water of less than 5°C or more than 50°/70°C enter the unit, this may damage the unit","(3) - Heating: 4 pipe: air 20°CDB, 15°CWB; entering water 65°C; leaving water 55°C","(3) - Do not let water of less than 5°C or more than 50°/70°C enter the unit, this may damage the unit","(3) - Heating: 4 pipe: air 20°CDB, 15°CWB; entering water 65°C; leaving water 55°C","(3) - Do not let water of less than 5°C or more than 50°/70°C enter the unit, this may damage the unit","(3) - Do not let water of less than 5°C or more than 50°/70°C enter the unit, this may damage the unit","(3) - Heating: 4 pipe: air 20°CDB, 15°CWB; entering water 65°C; leaving water 55°C"]
["","","","","","(4) - Height includes switch box","(4) - Height includes switch box","(4) - Height includes switch box","(4) - Height includes switch box","(4) - Height includes switch box","(4) - Height includes switch box","(4) - Height includes switch box","(4) - Height includes switch box"]
["","","","","","(5) - Do not let water of less than 5°C or more than 50°/70°C enter the unit, this may damage the unit","","(5) - Do not let water of less than 5°C or more than 50°/70°C enter the unit, this may damage the unit","","(5) - Do not let water of less than 5°C or more than 50°/70°C enter the unit, this may damage the unit","","","(5) - Do not let water of less than 5°C or more than 50°/70°C enter the unit, this may damage the unit"]