{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RY-CY1"]
[]
[]
[]
[]
["","","","","","RY90CY1M","RY125CY1M","RY140CY1M","RY160CY1M"]
["Refrigerant","Charge","","","kg","2.15","2.60","2.75","5.00"]
["","Type","","","","R-22","R-22","R-22","R-22"]
["Piping connections","Piping length","OU - IU","Max.","m","45","45","45","35"]
["","Level difference","IU - OU","Max.","m","25","25","25","15"]
["","Additional refrigerant charge","","","kg/m","Depending on distance (see manual)","Depending on distance (see manual)","Depending on distance (see manual)","Depending on distance (see manual)"]
["Dimensions","Unit","","Width","mm","1,030","1,030","1,030","1,030"]
["","","","Depth","mm","400","400","400","400"]
["","","","Height","mm","850","850","850","850"]
["Compressor","Type","","","","Scroll compressor","Scroll compressor","Scroll compressor","Scroll compressor"]
["Weight","Unit","","","kg","95","100","105","108"]
["Power supply","Phase","","","","3~","3~","3~","3~"]
["","Frequency","","","Hz","50","50","50","50"]
["","Voltage","","","V","380-415","380-415","380-415","380-415"]