{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":98,"n_cols":9,"rows_kept":98,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Faible niveau sonore de fonctionnement","dBA","","36","","41"]
["","","","Bas","dBA","","38","","43"]
["","Rafraîchissement","","Faible niveau sonore de fonctionnement","dBA","","36","","41"]
["","","","Bas","dBA","","38","","43"]
["","","","Haut","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Accessoires standard","Manuel d'installation","","","","","Manuel d'installation","","Manuel d'installation"]
["","Manuel d’utilisation","","","","","Manuel d’utilisation","","Manuel d’utilisation"]
["","Vis","","","","","Vis","","Vis"]
["","Rondelle","","","","","Rondelle","","Rondelle"]
["","Télécommande infrarouge","","","","","Télécommande infrarouge","","Télécommande infrarouge"]
["","Grille de verrouillage de protection","","","","","Grille de verrouillage de protection","","Grille de verrouillage de protection"]
["","Batterie","","","","","Batterie","","Batterie"]
["Systèmes de commande","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Piping connections","Liquide","","DE","mm","","9.52","","9.52"]
["","Gaz","","DE","mm","","15.88","","15.88"]
["","Évacuation","","","","","19.05","","19.05"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","0.094","","0.137"]
["","Chauffage","","Nom.","kW","","0.094","","0.137"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","56","","60"]
["","Chauffage","","","dBA","","56","","60"]
["Dimensions","Unité","","Largeur","mm","","820","","820"]
["","","","Profondeur","mm","","820","","820"]
["","","","Hauteur","mm","","300","","300"]
["Caisson","Matériau","","","","","Acier galvanisé","","Acier galvanisé"]
["Poids","Unité","","","kg","","39","","39"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","","29.2","","34.0"]
["","","","Bas","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Rafraîchissement","Bas","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","Haut","m³/min","","29.2","","34.0"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","17.6","","22.1"]
["","","Rafraîchissement","Faible niveau sonore de fonctionnement","m³/min","","17.6","","22.1"]
["Panneau décoratif","Poids","","","kg","","4","","4"]
["","Dimensions","","Hauteur","mm","","82","","82"]
["","","","Profondeur","mm","","990","","990"]
["","","","Largeur","mm","","990","","990"]
["","Couleur","","","","","Blanc","","Blanc"]
["Power supply","Phase","","","","","1~","","1~"]
["","Nom","","","","","V1","","V1"]
["","Fréquence","","","Hz","","50","","50"]
["","Tension","","","V","","220-240","","220-240"]
["Ventilateur","Débit d'air","Chauffage","Faible niveau sonore de fonctionnement","m³/min","15","","22.1"]
["Puissance absorbée","Chauffage","","Nom.","kW","0.067","","0.137"]
["","Rafraîchissement","","Nom.","kW","0.067","","0.137"]
["Ventilateur","Débit d'air","Rafraîchissement","Faible niveau sonore de fonctionnement","m³/min","15","","22.1"]
["Caisson","Matériau","","","","Acier galvanisé","","Acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","265","","300"]
["","","","Largeur","mm","820","","820"]
["","","","Profondeur","mm","820","","820"]
["Poids","Unité","","","kg","31","","39"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Bas","m³/min","17.6","","26.3"]
["","","Chauffage","Haut","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Bas","m³/min","17.6","","26.3"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","54","","60"]
["","Chauffage","","","dBA","54","","60"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Bas","dBA","35","","43"]
["","","","Faible niveau sonore de fonctionnement","dBA","32","","41"]
["","Chauffage","","Haut","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Bas","dBA","35","","43"]
["","","","Faible niveau sonore de fonctionnement","dBA","32","","41"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52","","9.52"]
["","Gaz","","DE","mm","15.88","","15.88"]
["","Évacuation","","","","19.05","","19.05"]
["Panneau décoratif","Couleur","","","","Blanc","","Blanc"]
["","Dimensions","","Hauteur","mm","82","","82"]
["","","","Largeur","mm","990","","990"]
["","","","Profondeur","mm","990","","990"]
["","Poids","","","kg","4","","4"]
["Systèmes de commande","Télécommande infrarouge","","","","ARCWLA","","ARCWLA"]
["","Télécommande câblée","","","","ARCWB","","ARCWB"]
["Accessoires standard","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Alimentation électrique","Nom","","","","V1","","V1"]
["","Phase","","","","1~","","1~"]
["","Fréquence","","","Hz","50","","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","","220-240"]