{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-R9"]
[]
[]
[]
[]
["","","","","ATXM25R2V1B / ARXM25R5V1B9","ATXM25R5V1B / ARXM25R5V1B9","ATXM35R2V1B / ARXM35R5V1B9","ATXM35R5V1B / ARXM35R5V1B9"]
["Puissance frigorifique","Min.","","kW","","","1.40"]
["","Max.","","kW","","","4.00"]
["","Nom.","","kW","","","3.40"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","","","402"]
["","EER","","","","","4.23"]
["","COP","","","","","4.04"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","","A"]
["","","Chauffage","","","","A"]
["Puissance calorifique","Nom.","","kW","","","4.00"]
["","Min.","","kW","","","1.40"]
["","Max.","","kW","","","5.20"]
["Remarques","","","","","","(1) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","","","(2) - Pour les données électriques, se reporter au schéma séparé."]
["","","","","","","(3) - Les puissances frigorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","","","(4) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["Puissance frigorifique","Min.","","kW","1.30","1.30","","1.40"]
["","Nom.","","kW","2.50","2.50","","3.40"]
["","Max.","","kW","3.20","3.20","","4.00"]
["Puissance calorifique","Puissance calorifique-=-Min.-=-kW","","kW","1.30","1.30","","1.40"]
["","Nom.","","kW","2.80","2.80","","4.00"]
["","Max.","","kW","4.70","4.70","","5.20"]
["Efficacité nominale","EER","","","4.50","4.50","","4.23"]
["","COP","","","5.00","5.00","","4.04"]
["","Consommation énergétique annuelle","","kWh","278","278","","402"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A","","A"]
["","","Chauffage","","A","A","","A"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A+++","A+++","","A+++"]
["","Puissance","Pdesign","kW","2.50","2.50","","3.40"]
["","SEER","","","8.55","8.55","","8.55"]
["","Consommation d’énergie annuelle","","kWh/a","102","102","","139"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A+++","A+++","","A+++"]
["","Puissance","Pdesign","kW","2.40","2.40","","2.50"]
["","SCOP/A","","","5.10","5.10","","5.10"]
["","Pdh Puissance calorifique à -10°","","kW","2.30","2.30","","2.35"]
["","Consommation d’énergie annuelle","","kWh/a","659","659","","686"]
["Classe d'efficacité énergétique","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]