{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":10,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-CB / ERLQ-CW1"]
[]
[]
[]
[]
["","","","","EHBH11CB3V / ERLQ011CAW1","EHBH11CB9W / ERLQ011CAW1","EHBH16CB9W / ERLQ014CAW1","EHBH16CB3V / ERLQ014CAW1","EHBH16CB9W / ERLQ016CAW1","EHBH16CB3V / ERLQ016CAW1"]
["COP","","","","4.60 (1), 2.75 (3), 3.55 (2), 2.10 (4)","4.60 (1), 2.75 (3), 3.55 (2), 2.10 (4)","4.30 (1), 2.65 (3), 3.32 (2), 2.08 (4)","4.30 (1), 2.65 (3), 3.32 (2), 2.08 (4)","4.25 (1), 2.64 (3), 3.26 (2), 2.09 (4)","4.25 (1), 2.64 (3), 3.26 (2), 2.09 (4)"]
["Puissance calorifique","Nom.","","kW","11.2 (1), 11.0 (2)","11.2 (1), 11.0 (2)","14.5 (1), 13.6 (2)","14.5 (1), 13.6 (2)","16.0 (1), 15.2 (2)","16.0 (1), 15.2 (2)"]
["","Max.","","kW","8.60 (3), 8.60 (4)","8.60 (3), 8.60 (4)","10.6 (3), 10.8 (4)","10.6 (3), 10.8 (4)","11.4 (3), 10.9 (4)","11.4 (3), 10.9 (4)"]
["Power input","Chauffage","Max.","kW","3.13 (3), 4.10 (4)","3.13 (3), 4.10 (4)","4.00 (3), 5.19 (4)","4.00 (3), 5.19 (4)","4.32 (3), 5.22 (4)","4.32 (3), 5.22 (4)"]
["","","Nom.","kW","2.43 (1), 3.10 (2)","2.43 (1), 3.10 (2)","3.37 (1), 4.10 (2)","3.37 (1), 4.10 (2)","3.76 (1), 4.66 (2)","3.76 (1), 4.66 (2)"]
["Remarques","","","","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - Condition 1 : rafraîchissement Ta 35 °C - LWE 18 °C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)","(2) - Condition 2 : rafraîchissement Ta 35 °C - LWE 7°C (DT = 5 °C) ; chauffage Ta BS/BH 7 °C/6 °C - LWC 45 °C (DT = 5 °C)"]
["","","","","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C","(3) - Condition 3 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 35 °C"]
["","","","","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C","(4) - Condition 4 : chauffage Ta BS -7 °C (HR : 85 %) - LWC 45 °C"]
["","","","","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C)","(5) - Tamb 35 °C - LWE 7 °C (DT=5 °C)"]
["","","","","(6) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(6) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(6) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(6) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(6) - Tamb 35 °C - LWE 18°C (DT=5 °C)","(6) - Tamb 35 °C - LWE 18°C (DT=5 °C)"]
["","","","","(7) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(7) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(7) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(7) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(7) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)","(7) - BS/BH 7 °C/6 °C-LWC 35 °C(DT=5 °C)"]
["","","","","(8) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(8) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(8) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(8) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(8) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)","(8) - BS/BH 7 °C/6 °C - LWC 45 °C(Dt=5 °C)"]