{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / AZAS-MV"]
[]
[]
[]
[]
["","","","","FBA100A2VEB / AZAS100MUV","FBA125A2VEB / AZAS125MUV","FBA140A2VEB / AZAS140MUV"]
["Puissance frigorifique","Nom.","","kW","9.5","12.1 (1)","13.4 (1)"]
["Puissance calorifique","Nom.","","kW","","13.5 (2)","15.5 (2)"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","A+"]
["","Puissance","Pdesign","kW","9.5","12.1","13.4"]
["","SEER","","","5.67","5.24","5.72"]
["","Consommation d’énergie annuelle","","kWh/a","586","1385","1406"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","A"]
["","Puissance","Pdesign","kW","6","6","7.8"]
["","SCOP/A","","","3.81","3.55","3.85"]
["","Consommation d’énergie annuelle","","kWh/a","2205","2366","2836"]
["Remarques","","","","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m.","(1) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Puissance calorifique","Nom.","","kW","10.8 (2)"]