{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RQ-BV3"]
[]
[]
[]
[]
["","","","","FBA100A2VEB / RQ100B8V3B"]
["Puissance frigorifique","Nom.","","kW","10.0 (1)"]
["Efficacité nominale","EER","","","2.61"]
["","Consommation énergétique annuelle","","kWh","1,915"]
["","COP","","","2.99"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","D"]
["","","Chauffage","","D"]
["Puissance calorifique","Nom.","","kW","11.2 (4)"]
["Remarques","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 5m ; dénivelé : 0m"]
["","","","","(2) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m (horizontale) ; dénivelé : 0m"]
["","","","","(3) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m"]
["","","","","(4) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 5m ; dénivelé : 0m"]
["","","","","(5) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m"]