{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":12,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D"]
[]
[]
[]
[]
["","","","","","FBQ35D2VEB (Archived)","FBQ50D2VEB (Archived)","FBQ60D2VEB (Archived)","FBQ71D2VEB (Archived)","FBQ100D2VEB (Archived)","FBQ125D2VEB (Archived)","FBQ140D2VEB (Archived)"]
["Ventilateur","Pression statique externe","","Haute","Pa","150","150","150","150","150","150","150"]
["Caisson","Couleur","","","","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)","Non peinte (galvanisée)"]
["","Matériau","","","","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé","Tôle en acier galvanisé"]
["Dimensions","Unité","","Hauteur","mm","245","245","245","245","245","245","245"]
["","","","Largeur","mm","700","700","1000","1000","1400","1400","1400"]
["","","","Profondeur","mm","800","800","800","800","800","800","800"]
["Poids","Unité","","","kg","28","28","35","35","46","46","46"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","15","15","18","18","29","34","34"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","12.5","12.5","15","15","26","29","29"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","10.5","10.5","12.5","12.5","23","23.5","23.5"]
["","","Chauffage","Haut","m³/min","15","15","18","18","29","34","34"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","12.5","12.5","15","15","26","29","29"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","10.5","10.5","12.5","12.5","23","23.5","23.5"]
["","Pression statique externe","","Nom.","Pa","30","30","30","30","40","50","50"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","60","60","56","56","58","62","62"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","35","35","30","30","34","37","37"]
["","Refroidissement","","Moyen","dBA","32","32","28","28","32","35","35"]
["","","","Bas","dBA","29","29","25","25","30","32","32"]
["","Chauffage","","Haut","dBA","37","37","31","31","36","38","38"]
["","","","Moyen","dBA","34","34","28","28","33","35","35"]
["","","","Bas","dBA","29","29","25","25","30","32","32"]
["Réfrigérant","Réfrigérant-=-PRP","","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gaz","","DE","mm","9.52","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Évacuation","","","","VP20 (D.I. 20/D.E. 26), hauteur de refoulement 625 mm","VP20 (D.I. 20/D.E. 26), hauteur de refoulement 625 mm","VP20 (D.I. 20/D.E. 26), hauteur de refoulement 625 mm","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Hauteur manométrique","mm","","","","625","625","625","625","625","625","625"]
["Systèmes de commande","Télécommande infrarouge","","","","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["","Télécommande câblée","","","","","","","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528","BRC1E52A/B, BRC1D528"]
["Accessoires standard","Installation manual","","","","1","1","1","1","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","8","8","8","8"]
["","Operation manual","","","","1","1","1","1","1","1","1"]
["","Clamps","","","","4","4","4","4","4","4","4"]
["","Drain hose","","","","1","1","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","1","1","1","1"]
["","Screws","","","","40","40","40","40","40","40","40"]
["","Sealing pad","","","","5","5","5","5","5","5","5"]
["","Sealing pads","","","","","","","5","5","5","5"]
["Alimentation électrique","Nom","","","","VE","VE","VE","VE","VE","VE","VE"]
["","Phase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240","220-240/220","220-240/220","220-240/220","220-240/220"]
["Remarques","","","","","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore.","(1) - Le niveau de puissance sonore est une valeur absolue indiquant la puissance générée par une source sonore."]