{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RQ-BW1"]
[]
[]
[]
[]
["","","","","FHA71AVEB / RQ71B8W1B","FHA100AVEB / RQ100B8W1B","FHA125AVEB / RQ125B8W1B"]
["Puissance frigorifique","Nom.","","kW","7.10 (2)","9.80 (2)","12.2 (1)"]
["Piping connections","Liquide","DE","mm","9.52","9.52","9.52"]
["","Gaz","DE","mm","15.9","15.9","15.9"]
["","Évacuation","DE","mm","26","26","26"]
["Efficacité nominale","EER","","","2.68","2.66","2.71"]
["","Consommation énergétique annuelle","","kWh","1,325","1,840","2,255"]
["","COP","","","2.86","2.79","2.81"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","D","D","D"]
["","","Chauffage","","D","E","D"]
["Puissance calorifique","Nom.","","kW","8.00 (3)","11.2 (3)","14.5 (3)"]
["Remarques","","","","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m","(1) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m (horizontale) ; dénivelé : 0m"]
["","","","","(2) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m (horizontale) ; dénivelé : 0m","(2) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m (horizontale) ; dénivelé : 0m","(2) - Rafraîchissement : temp. intérieure  27 °CBS, 19 °CBH ; temp. extérieure 35 °CBS ; longueur équivalente de tuyauterie : 7,5m ; dénivelé : 0m"]
["","","","","(3) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m","(3) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m","(3) - Chauffage : temp. intérieure  20 °CBS ; temp. extérieure 7 °CBS, 6 °CBH ; tuyauterie équivalente de réfrigérant : 7,5m ; dénivelé : 0m"]