{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Puissance frigorifique","Nom.","","kW","3.40"]
["Rafraîchissement de l'air ambiant","SEER","","","6.24"]
["","Consommation d’énergie annuelle","","kWh/a","191"]
["","Puissance","Pdesign","kW","3.40"]
["","Classe d’efficacité énergétique","","","A++"]
["Chauffage des locaux (climat tempéré)","Puissance","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Classe d’efficacité énergétique","","","A+"]
["","Consommation d’énergie annuelle","","kWh/a","979"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","456"]
["","EER","","","3.73"]
["","COP","","","4.08"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A"]
["","","Chauffage","","A"]
["Puissance calorifique","Nom.","","kW","4.00"]
["Remarques","","","","(1) - Pour les données électriques, se reporter au schéma séparé."]
["","","","","(2) - Voir le schéma séparé pour la plage de fonctionnement"]
["","","","","(3) - Les puissances frigorifiques nom. sont basées sur les valeurs suivantes : température intérieure : 27 °CBS, 19 °CBH ; température extérieure : 35°C BS ; longueur équivalente de tuyauterie de réfrigérant : 5 m, dénivellation : 0 m."]
["","","","","(4) - Les puissances calorifiques nominales sont basées sur les valeurs suivantes : température intérieure : 20°CBS ; température extérieure : 7°CBS, 6°CBH, longueur de tuyauterie de réfrigérant équivalente : 5m, dénivelé : 0 m."]
["Unité extérieure","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Puissance frigorifique","Nom.","","kW","","5.00","5.70"]
["Puissance calorifique","Nom.","","kW","","6.00","7.20"]
["Efficacité nominale","EER","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Consommation énergétique annuelle","","kWh","","780","867"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","","B","A"]
["","","Chauffage","","","C","C"]
["Rafraîchissement des locaux","Classe d’efficacité énergétique","","","","A+","A+"]
["","Puissance","Pdesign","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Consommation d’énergie annuelle","","kWh/a","","295","328"]
["Chauffage des locaux (climat tempéré)","Classe d’efficacité énergétique","","","","A","A"]
["","Puissance","Pdesign","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Pdh Puissance calorifique à -10°","","kW","","3.85","4.08"]
["","Consommation d’énergie annuelle","","kWh/a","","1578","1704"]