{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RXS-L"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / RXS35L2V1B","FHQ50CAVEB / RXS50L2V1B","FHQ60CAVEB / RXS60L2V1B"]
["Puissance frigorifique","Min.","","kW","1.4","1.7","1.7"]
["","Max.","","kW","4.0","5.3","5.7"]
["","Nom.","","kW","3.40","5.0","5.7"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35","6.35"]
["","Gaz","DE","mm","9.5","12.7","12.7"]
["","Évacuation","DE","mm","VP20","VP20 (diamètre ext. : 26 / diamètre int. : 20)","VP20 (diamètre ext. : 26 / diamètre int. : 20)"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","475","785","875"]
["","EER","","","3.58","3.18","3.26"]
["","COP","","","4.08","3.35","3.32"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","B","A"]
["","","Chauffage","","A","C","C"]
["Puissance calorifique","Nom.","","kW","4.00","6.0","7.20"]
["","Min.","","kW","1.3","1.7","1.7"]
["","Max.","","kW","5.1","6.0","7.2"]
["Remarques","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(2) - 220V","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230 V","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240V","(4) - 240V","(4) - 240V"]
["","","","","(5) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(5) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(5) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]