{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":9,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BW","FTXJ25MV1BW","FTXJ35MV1BW","FTXJ50MV1BW"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.023","0.023","0.033","0.033"]
["","Chauffage","","Nom.","kW","0.031","0.033","0.042","0.043"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","303","303","303","303"]
["","","","Largeur","mm","998","998","998","998"]
["","","","Profondeur","mm","212","212","212","212"]
["Poids","Unité","","","kg","12","12","12","12"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","8.9","8.9","10.9","10.9"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","6.6","6.6","7.8","8.9"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","4.4","4.4","4.8","6.8"]
["","","","Faible niveau sonore de fonctionnement","m³/min","2.6","2.6","2.9","3.6"]
["","","Chauffage","Haut","m³/min","10.2","11.0","12.4","12.6"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","8.4","8.6","9.6","10.5"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","6.3","6.3","6.9","8.1"]
["","","","Faible niveau sonore de fonctionnement","m³/min","3.8","3.8","4.1","5.0"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","54","54","59","60"]
["","Chauffage","","","dBA","56","56","59","60"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","38","38","45","46"]
["","Refroidissement","","Moyen","dBA","32","32","34","40"]
["","","","Bas","dBA","25","25","26","35"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","19","20","25"]
["","Chauffage","","Haut","dBA","40","41","45","47"]
["","","","Moyen","dBA","34","34","37","41"]
["","","","Bas","dBA","28","28","29","35"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","19","20","25"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35","6.35"]
["","Gaz","","DE","mm","9.50","9.50","9.50","12.70"]
["","Évacuation","","","","18","18","18","18"]
["Control systems","Infrared remote control","","","","ARC466A9","ARC466A9","ARC466A9","ARC466A9"]
["Accessoires standard","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","Screw cover","","","","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Fixing screw for remote controller holder","","","","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2","2"]
["","Fixing screws for mounting plate","","","","5","5","5","5"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Alimentation électrique","Nom","","","","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240","220-240"]
["Remarques","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]