{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":8,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXN-L / RXN-L"]
[]
[]
[]
[]
["","","","","FTXN25LV1B / RXN25LV1B","FTXN35LV1B / RXN35LV1B","FTXN50LV1B / RXN50LV1B","FTXN60LV1B / RXN60LV1B"]
["Puissance frigorifique","Min.","","kW","1.30","1.30","1.88","2.00"]
["","Max.","","kW","2.80","3.50","6.20","6.50"]
["","Nom.","","kW","2.50","3.20","5.45","6.21"]
["Raccords de tuyauterie","Liquide","DE","mm","6.35","6.35","6.35","6.35"]
["","Gaz","DE","mm","9.52","9.52","12.70","15.90"]
["","Évacuation","DE","mm","16.5","16.5","16.5","16.5"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","390","498","850","965"]
["","EER","","","3.21","3.22","3.21","3.22"]
["","COP","","","3.61","3.61","3.61","3.62"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A","A","A"]
["","","Chauffage","","A","A","A","A"]
["Puissance calorifique","Nom.","","kW","2.80","3.50","5.62","6.40"]
["","Min.","","kW","1.30","1.30","1.32","1.56"]
["","Max.","","kW","3.70","4.00","6.60","7.10"]
["Remarques","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]