{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","40","","","","","","45"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","","","","","","22"]
["","","","Bas","dBA","27","","","","","","33"]
["","Rafraîchissement","","Faible niveau sonore de fonctionnement","dBA","19","","","","","","21"]
["","","","Bas","dBA","24","","","","","","33"]
["","","","Haut","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Rafraîchissement","","Nom.","dBA","32","","","","","","39"]
["Accessoires standard","Manuel d'installation","","","","1","","","","","","1"]
["","Manuel d’utilisation","","","","1","","","","","","1"]
["","Télécommande infrarouge","","","","1","","","","","","1"]
["","Piles","","","","2","","","","","","2"]
["","Support de télécommande","","","","1","","","","","","1"]
["","Plaque de montage","","","","1","","","","","","1"]
["","Vis de fixation d'unité intérieure","","","","2","","","","","","2"]
["","Filtre purificateur d'air photocatalytique à apatite de titane","","","","2","","","","","","2"]
["Systèmes de commande","Télécommande infrarouge","","","","ARC466A6","","","","","","ARC466A6"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","","","","","","6.35"]
["","Gaz","","DE","mm","9.5","","","","","","9.5"]
["","Évacuation","","","","18","","","","","","18"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Chauffage","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","58","","","","","","59"]
["","Chauffage","","","dBA","58","","","","","","59"]
["Dimensions","Unité","","Largeur","mm","780","","","","","","900"]
["","","","Profondeur","mm","215","","","","","","215"]
["","","","Hauteur","mm","289","","","","","","298"]
["Caisson","Couleur","","","","Blanc","","","","","","Blanc"]
["Poids","Unité","","","kg","8","","","","","","11"]
["Power supply","Phase","","","","1~","","","","","","1~"]
["","Fréquence","","","Hz","50","","","","","","50"]
["","Nom","","","","V1","","","","","","V1"]
["","Tension","","","V","220-240","","","","","","220-240"]
["Remarques","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - En cas de connexion à l’unité extérieure du système Multi, se reporter aux caractéristiques techniques de l’unité extérieure de type Multi à raccorder.","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230 V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Chauffage","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Caisson","Couleur","","","","","Blanc","Blanc","Blanc","Blanc","Blanc","","Blanc","Blanc","Blanc"]
["Dimensions","Unité","","Hauteur","mm","","215","289","215","298","215","","215","298","215"]
["","","","Largeur","mm","","780","780","780","900","900","","900","900","900"]
["","","","Profondeur","mm","","289","215","289","215","298","","298","215","298"]
["Poids","Unité","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["Ventil.","Débit d'air","Refroidissement","Moyen","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["Ventilateur","Débit d'air","Rafraîchissement","Bas","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Chauffage","Haut","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["Ventil.","Débit d'air","Chauffage","Moyen","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["Ventilateur","Débit d'air","Chauffage","Bas","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Faible niveau sonore de fonctionnement","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Chauffage","","","dBA","","58","58","58","59","59","","59","60","60"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","","40","41","41","45","45","","45","46","46"]
["","Refroidissement","","Moyen","dBA","","32","33","33","","37","","39","","40"]
["","","","Bas","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Faible niveau sonore de fonctionnement","dBA","","19","19","19","19","19","","21","23","23"]
["","Chauffage","","Haut","dBA","","40","41","41","45","45","","45","47","47"]
["","","","Moyen","dBA","","34","34","34","","39","","39","","40"]
["","","","Bas","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Faible niveau sonore de fonctionnement","dBA","","19","19","19","19","19","","22","24","24"]
["Raccords de tuyauterie","Liquide","","DE","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gaz","","DE","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Évacuation","","","","","18","18","18","18","18","","18","18","18"]
["Systèmes de commande","Télécommande infrarouge","","","","","ARC466A6","","","","","","ARC466A9"]
["Accessoires standard","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Alimentation électrique","Nom","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Phase","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Fréquence","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilateur","Débit d'air","Rafraîchissement","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","","","33","","37","","","","40"]
["Ventilateur","Débit d'air","Chauffage","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","","","34","","39","","","","40"]
["Systèmes de commande","Télécommande infrarouge","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Accessoires standard","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Remarques","","","","","","","","","","","(4) - 240V"]