{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","39","42","44"]
["","","","Faible niveau sonore de fonctionnement","dBA","19","19","24"]
["","","","Bas","dBA","28","29","31"]
["","Rafraîchissement","","Faible niveau sonore de fonctionnement","dBA","19","19","23"]
["","","","Bas","dBA","26","27","30"]
["","","","Haut","dBA","38","42","47"]
["","","","Nom.","dBA","35","36","38"]
["","Rafraîchissement","","Nom.","dBA","33","35","38"]
["Accessoires standard","Filtre désodorisant et purificateur d'air photocatalytique","","","","1","1","1"]
["","Télécommande infrarouge","","","","1","1","1"]
["","Piles sèches","","","","2","2","2"]
["","Support de télécommande","","","","1","1","1"]
["","Vis de fixation d'unité intérieure","","","","3","3","3"]
["","Plaque de montage","","","","1","1","1"]
["Systèmes de commande","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Raccords de tuyauterie","Liquide","","DE","mm","6.35","6.35","6.35"]
["","Gaz","","DE","mm","9.5","9.5","9.5"]
["Puissance absorbée","Rafraîchissement","","Nom.","kW","0.030","0.030","0.030"]
["","Chauffage","","Nom.","kW","0.030","0.030","0.030"]
["Sound power level","Rafraîchissement","","","dBA","54","57","60"]
["","Chauffage","","","dBA","56","57","59"]
["Dimensions","Unité","","Largeur","mm","798","798","798"]
["","","","Profondeur","mm","372","372","372"]
["","","","Hauteur","mm","295","295","295"]
["Caisson","Couleur","","","","Blanc","Blanc","Blanc"]
["Poids","Unité","","","kg","15","15","15"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","11.7","13.3","14.4"]
["","","","Bas","m³/min","6.7","6.9","7.7"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.8","4.8","5.9"]
["","","Rafraîchissement","Bas","m³/min","5.3","5.6","6.6"]
["","","","Haut","m³/min","10.7","12.1","15.0"]
["","","","Faible niveau sonore de fonctionnement","m³/min","4.0","4.0","4.6"]
["","","","Nom.","m³/min","8.6","9.2","10.7"]
["","","Rafraîchissement","Nom.","m³/min","7.5","8.4","9.2"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Nom","","","","V1","V1","V1"]
["","Fréquence","","","Hz","50","50","50"]
["","Tension","","","V","220-240","220-240","220-240"]
["Remarques","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Avant de l'échangeur de chaleur","(4) - Avant de l'échangeur de chaleur","(4) - Avant de l'échangeur de chaleur"]
["","","","","","(5) - Arrière de l'échangeur de chaleur","(5) - Arrière de l'échangeur de chaleur","(5) - Arrière de l'échangeur de chaleur"]