{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTY-HL"]
[]
[]
[]
[]
["","","","","","FTY18HEVLK","FTY24HEVLK","FTY30HEVLK"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","44","45"]
["","","","Faible niveau sonore de fonctionnement","dBA","35","32"]
["","","","Bas","dBA","38","37"]
["","Rafraîchissement","","Faible niveau sonore de fonctionnement","dBA","33","34"]
["","","","Bas","dBA","36","37"]
["","","","Haut","dBA","44","45"]
["","","","Nom.","dBA","40","40","44"]
["","Rafraîchissement","","Nom.","dBA","40","42","44"]
["Dimensions","Unité","","Largeur","mm","940","1,007","1,178"]
["","","","Profondeur","mm","298","219","227"]
["","","","Hauteur","mm","200","315","326"]
["Poids","Unité","","","kg","13","15.5","17.5"]
["Ventilateur","Débit d'air","Chauffage","Haut","m³/min","780","800"]
["","","","Bas","m³/min","550","600"]
["","","Rafraîchissement","Bas","m³/min","550","600"]
["","","","Haut","m³/min","780","800"]
["","","","Nom.","m³/min","650","700"]
["","","Rafraîchissement","Nom.","m³/min","650","700"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","60","60","60"]
["","Nom","","","","VL","VL","VL"]
["","Tension","","","V","220","220","220"]