{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":9,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","","FVQ71CVEB (Archived)","FVQ100CVEB (Archived)","FVQ125CVEB (Archived)","FVQ140CVEB (Archived)"]
["Puissance absorbée","Chauffage","","Nom.","kW","0.117","0.238","0.238","0.276"]
["","Rafraîchissement","","Nom.","kW","0.117","0.238","0.238","0.276"]
["Caisson","Couleur","","","","Blanc frais","Blanc frais","Blanc frais","Blanc frais"]
["Dimensions","Unité","","Hauteur","mm","1850","1850","1850","1850"]
["","","","Largeur","mm","600","600","600","600"]
["","","","Profondeur","mm","270","350","350","350"]
["Poids","Unité","","","kg","39","47","47","47"]
["Ventilateur","Débit d'air","Rafraîchissement","Haut","m³/min","18","28","28","30"]
["","","","Nom.","m³/min","16","25","26","28"]
["","","","Bas","m³/min","14","22","24","26"]
["","","Chauffage","Haut","m³/min","18","28","28","30"]
["","","","Nom.","m³/min","16","25","26","28"]
["","","","Bas","m³/min","14","22","24","26"]
["Niveau de puissance sonore","Rafraîchissement","","","dBA","55","62","63","65"]
["","Chauffage","","","dBA","55","62","63","65"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","43","50","51","53"]
["","","","Nom.","dBA","41","47","48","51"]
["","","","Bas","dBA","38","44","46","48"]
["","Chauffage","","Haut","dBA","43","50","51","53"]
["","","","Nom.","dBA","41","47","48","51"]
["","","","Bas","dBA","38","44","46","48"]
["Raccords de tuyauterie","Liquide","","DE","mm","9.52","9.52","9.52","9.52"]
["","Gaz","","DE","mm","15.9","15.9","15.9","15.9"]
["","Évacuation","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Systèmes de commande","Télécommande câblée","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Accessoires standard","Installation manual","","","","Installation manual","Installation manual","Installation manual","Installation manual"]
["","Hole protection rubber","","","","Hole protection rubber","Hole protection rubber","Hole protection rubber","Hole protection rubber"]
["","Cover","","","","Cover","Cover","Cover","Cover"]
["","Dew proof material","","","","Dew proof material","Dew proof material","Dew proof material","Dew proof material"]
["","Remote control wiring","","","","Remote control wiring","Remote control wiring","Remote control wiring","Remote control wiring"]
["","Bracket for installation","","","","Bracket for installation","Bracket for installation","Bracket for installation","Bracket for installation"]
["","Operation manual","","","","Operation manual","Operation manual","Operation manual","Operation manual"]
["","Bush","","","","Bush","Bush","Bush","Bush"]
["","Clamps","","","","Clamps","Clamps","Clamps","Clamps"]
["","Installation pattern","","","","Installation pattern","Installation pattern","Installation pattern","Installation pattern"]
["","Insulation for fitting","","","","Insulation for fitting","Insulation for fitting","Insulation for fitting","Insulation for fitting"]
["","Screws","","","","Screws","Screws","Screws","Screws"]
["Alimentation électrique","Phase","","","","1~","1~","1~","1~"]
["","Fréquence","","","Hz","50/60","50/60","50/60","50/60"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]