{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXS-F / RXS-L3"]
[]
[]
[]
[]
["","","","","FVXS25FV1B / RXS25L3V1B","FVXS35FV1B / RXS35L3V1B"]
["Puissance frigorifique","Min.","","kW","1.3","1.4"]
["","Max.","","kW","3.0","3.8"]
["","Nom.","","kW","2.5 (2)","3.5 (2)"]
["Piping connections","Liquide","DE","mm","6.35","6.35"]
["","Gaz","DE","mm","9.5","9.5"]
["","Évacuation","DE","mm","20.0","20.0"]
["Efficacité nominale","Consommation énergétique annuelle","","kWh","303","530"]
["","EER","","","4.12 (1)","3.30 (1)"]
["","COP","","","4.42 (1)","3.78 (1)"]
["","Directive sur l'étiquetage énergétique","Rafraîchissement","","A","A"]
["","","Chauffage","","A","A"]
["Puissance calorifique","Nom.","","kW","3.4 (2)","4.5 (2)"]
["","Min.","","kW","1.3","1.4"]
["","Max.","","kW","4.5","5.0"]
["Remarques","","","","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement","(1) - Valeurs EER/COP conformes à la norme Eurovent 2012, pour utilisation hors UE uniquement"]
["","","","","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°","(2) - Efficacité nominale : rafraîchissement à charge nominale 35°/27°, chauffage à charge nominale 7°/20°"]
["","","","","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240V","(5) - 240V"]