{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXN-MB"]
[]
[]
[]
[]
["","","","","","RXN25MV1B","RXN35MV1B","RXN50MV1B","RXN60MV1B"]
["Niveau de pression sonore","Chauffage","","Nom.","dBA","","","","51"]
["","Rafraîchissement","","Nom.","dBA","","","","51"]
["Réfrigérant","Charge","","","TCO2Eq","","","","3"]
["","PRP","","","","","","","2,087.5"]
["","Charge","","","kg","","","","1.45"]
["","Type","","","","","","","R-410A"]
["Compresseur","Type","","","","","","","Swing hermétique"]
["Dimensions","Unité","","Largeur","mm","","","","855"]
["","","","Profondeur","mm","","","","328"]
["","","","Hauteur","mm","","","","753"]
["Poids","Unité","","","kg","","","","44"]
["Power supply","Phase","","","","","","","1~"]
["","Fréquence","","","Hz","","","","50"]
["","Tension","","","V","","","","220-240"]
["Remarques","","","","","","","","(1) - Toutes les caractéristiques techniques sont sujettes à modification par le fabricant sans préavis."]
["","","","","","","","","(2) - Contient des gaz à effet de serre fluorés."]
["Dimensions","Unité","","Hauteur","mm","550","550","753"]
["","","","Largeur","mm","658","658","855"]
["","","","Profondeur","mm","289","289","328"]
["Poids","Unité","","","kg","31","31","44"]
["Compresseur","Type","","","","Swing hermétique","Swing hermétique","Swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","10","10","-10"]
["","","","Max.","°CBS","46","46","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","-15","-15","-15"]
["","","","Max.","°CBH","18","18","18"]
["Niveau de pression sonore","Rafraîchissement","","Nom.","dBA","45","46","51"]
["","Chauffage","","Nom.","dBA","45","46","51"]
["Réfrigérant","","","","","R-410A","R-410A","R-410A"]
["","Charge","","","kg","1.00","1.00","1.45"]
["","Charge","","","tCO2Eq","2.1","2.1","3"]
["","Réfrigérant-=-PRP","","","","2087.5","2087.5","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","20","20","30"]
["Alimentation électrique","Phase","","","","1~","1~","1~"]
["","Fréquence","","","Hz","50","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240","220-240"]