{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Niveau de pression sonore","Chauffage","","Haut","dBA","","","48"]
["","Rafraîchissement","","Haut","dBA","","","48"]
["Accessoires standard","Manuel d'installation","","","","","","1"]
["","Étiquette de charge de réfrigérant","","","","","","1"]
["","Étiquettes multilingues de gaz à effet de serre fluorés","","","","","","1"]
["","Bouchon d'évacuation (modèles pompe à chaleur uniquement)","","","","","","1"]
["Réfrigérant","Charge","","","TCO2Eq","","","2.5"]
["","PRP","","","","","","2,087.5"]
["","Charge","","","kg","","","1.2"]
["","Type","","","","","","R-410A"]
["Moteur de ventil.","Vitesse","Rafraîchissement","Extra lent","tr/min","","","780"]
["","","Chauffage","Très lent","tr/min","","","740"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Max.","°CBS","","","46"]
["","","","Min.","°CBS","","","-10"]
["","Chauffage","Extérieure","Max.","°CBH","","","18"]
["","","","Min.","°CBH","","","-15"]
["Raccordements de tuyauterie","Dénivelé","UI - UE","Max.","m","","","15"]
["","Charge de réfrigérant supplémentaire","","","kg/m","","","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["Dimensions","Unité","","Largeur","mm","","","765"]
["","","","Profondeur","mm","","","285"]
["","","","Hauteur","mm","","","550"]
["Compresseur","Type","","","","","","Compresseur swing hermétique"]
["Poids","Unité","","","kg","","","34"]
["Ventilateur","Débit d'air","Chauffage","Très lent","cfm","","","904"]
["","","","Très lent","m³/min","","","25.6"]
["","","Rafraîchissement","Extra lent","m³/min","","","30.1"]
["","","","Extra lent","cfm","","","1,063"]
["Power supply","Phase","","","","","","1~"]
["","Fréquence","","","Hz","","","50"]
["","Tension","","","V","","","220-240"]
["Remarques","","","","","","","(1) - SL : Très faible niveau sonore de ventilation (réglage du débit d’air)"]
["Ventilateur","Débit d’air","Rafraîchissement","Extra lent","m³/min","30.1","30.1"]
["","","Chauffage","Très lent","m³/min","25.6","25.6"]
["","","","Extra lent","cfm","1063","1063"]
["","","Chauffage","Très lent","cfm","904","904"]
["Dimensions","Unité","","Hauteur","mm","550","550"]
["","","","Largeur","mm","765","765"]
["","","","Profondeur","mm","285","285"]
["Poids","Unité","","","kg","34","34"]
["Moteur de ventilateur","Vitesse","Rafraîchissement","Extra lent","tr/min","780","780"]
["","","Chauffage","Très lent","tr/min","740","740"]
["Compresseur","Type","","","","Compresseur swing hermétique","Compresseur swing hermétique"]
["Plage de fonctionnement","Rafraîchissement","Temp. ext.","Min.","°CBS","-10","-10"]
["","","","Max.","°CBS","46","46"]
["","Chauffage","Temp. ext.","Min.","°CBH","-15","-15"]
["","","","Max.","°CBH","18","18"]
["Niveau de pression sonore","Rafraîchissement","","Haut","dBA","46","46"]
["","Chauffage","","Haut","dBA","47","47"]
["Réfrigérant","","","","","R-410A","R-410A"]
["","Charge","","","kg","1.0","1.0"]
["","Charge","","","tCO2Eq","2.1","2.1"]
["","Réfrigérant-=-PRP","","","","2087.5","2087.5"]
["Raccords de tuyauterie","Longueur de tuyauterie","Max.","UE - UI","m","20","20"]
["","Charge de réfrigérant supplémentaire","","","kg/m","0,02 (pour longueur de tuyauterie supérieure à 10 m)","0,02 (pour longueur de tuyauterie supérieure à 10 m)"]
["","Dénivelé","UI - UE","Max.","m","15","15"]
["Accessoires standard","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Alimentation électrique","Phase","","","","1~","1~"]
["","Fréquence","","","Hz","50","50"]
["","Alimentation électrique-=-Tension-=-V","","","V","220-240","220-240"]
["Remarques","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]
["Accessoires standard","Drain plug (only heat pump models)","","","","","1"]